（警告：シングルガスバーナーの風防として使用しないでください。ガス容器が加熱され、ガス容器の内圧が上昇し、ガス漏れが生じたり、暴発の危険があります。また、熱がこもり容器の故障の原因となります。）

（各部の名称）

ゴトク

目皿

炭受け（固定金具）

本体（差し込み穴）

（ゴトクを使用する場合）

フレームが下、ワイヤーが上になる向きでセットしてください。

ワイヤー

フレーム

固定ワイヤー

ワイヤー

フレーム

品質表示

本体・炭受け：ステンレス銅

ゴトク・目皿：ステンレス銅

収納ケース：ポリエステル

組立サイズ（約）157ｘ195ｘ182ｍｍ

収納ケースサイズ（約）250ｘ195ｍｍ

■組立方法

①平坦で安全な場所を選び、部品を全部取り出します。図のように、本体がコの字になるように広げてください。

②炭受けは、燃料や用途に合わせ3段階にセットできます。炭受けの固定金具を本体側面の差し込み穴に通してセットしてください。

※炭受けは傾きなく、左右平行にセットしてください。※本体をひっくり返して上の差し込み穴にセットすると高くなります。

　⓵低

　⓶中

　⓷高

　本体をひっくり返して

③目皿の凸部を下向きにして、炭受けの中に入れてください。

④ゴトクの固定ワイヤーを本体側面の溝にセットしてください。

■収納方法

①図のように本体を開きます。

②炭受けの中に目皿を入れ、本体の真ん中の面にのせ、左側の面を畳みます。

③次に右面を畳みます。

④ゴトクと一緒にケースに収納できます。

　収納ケース

■燃料の着火方法

①目皿の上に適量の燃料を置いて着火してください。

（燃料の目安）

※木炭や薪等の燃料は重なるように置き、本体の側面に著しく触れないようにしてください。

※着火剤を使用する場合は燃料の下に入れて（敷いて）着火してください。●注意/使用する燃料や着火剤の注意事項をよく読んで、火傷等に充分注意してください。

②火がおきて火力が安定したら、用途に合わせてゴトクをセットしてください。

お問い合わせ

Skaterスケーター株式会社　消費者サービス係

〒630‐8520　奈良市否町216‐1

TEL(0742)63-2040

受付時間：10：00～12：00/13：00～17：00

（土日祝日は除きます）

■当社製品をご使用になったご感想やご意見、また、商品化を希望するアイデア等ございましたら、弊社企画部までお寄せください。採用・参考にさせていただいた場合には、寸志を贈らせていただきます。

FAX(0742)63-2041

(Warning: Do not use it as a windshield for a single gas burner. The gas container is heated, the internal pressure of the gas container rises, gas leakage occurs, there is a risk of explosion. In addition, heat will cause the failure of the appliance.）

(Name of each part)

Gotoku trivet

Mezara net

Charcoal tray (Fixing bracket)

Main body (Insertion hole)

(When using the Gotoku trivet)

Set the frame facing down and the wire facing up.

Wire

Frame

Fixing wire

Wire

Frame

Quality Indication

Main body, Charcoal tray: Stainless copper

Gotoku trivet, Mezara net: Stainless copper

Storage case: Polyester

Assembled size (approx.)157ｘ195ｘ182ｍｍ

Storage case size (approx.)250ｘ195ｍｍ

■How To Assemble

① Take out all the parts. Locate a flat, safe place and unfold the main body into a U-shape as shown in the illustration.

② The charcoal tray is set in 3 positions depending on the fuel and application. Set the charcoal tray by inserting the fixing bracket into the insertion hole on the side of the main body.

※Set the charcoal tray parallel to the left and right without tilting. ※Turn the main body over and set it in the upper insertion hole; the height will increase.

　⓵ Low

　⓶ Medium

　⓷ High

　Turn the main body over

③ Place the Mezara net in the charcoal tray with the protruding part facing downward.

④ Set the fixing wire of the Gotoku trivet into the slot on the side of the main body.

■How To Store

① Open the main body as shown in the illustration.

② Put the Mezara net in the charcoal tray, place them on the center of the main body, and fold the left side of the main body to the center.

③ Then fold the right side to the center.

④ Store in the case with the Gotoku trivet.

　Storage case

■How To Ignite Fuel

① Place an appropriate amount of fuel on the Mezara net and ignite it.

(Suggested amount of fuel)

※Fuel such as charcoal or firewood should be placed in layers and should not excessively touch the sides of the main body.

※If using a fire lighter, place (spread) it under the fuel to ignite it. ●Caution/Read the instructions for fuel and fire lighters carefully, and be careful of burns, etc.

② Once the fire starts and the heat stabilizes, set the Gotoku trivet according to your application.

Contact Us

SkaterSkater Co., Ltd. Consumer Service Section

Postal Code 630‐8520, 216-1 Karamomocho, Nara City

TEL (0742) 63-2040

Office Hours：10:00 - 12:00/13:00 - 17:00

(Excluding weekends and national holidays)

■If you have any feedback or opinions about our products or any ideas you would like to request for merchandising, please send them to our Planning Section. We will send you a small token of appreciation if we adopt or refer to your idea.

FAX (0742) 63-2041