Warning

Do not use it as a windshield for a single gas burner. The gas container heats up, increasing the internal pressure of the gas container, causing gas leakage and risk of explosion. It can also overheat and damage the equipment.

Gotoku trivet

Mezara net

Charcoal tray

Main body

How To Assemble

1. Take out all the parts. Locate a flat, safe place and unfold the main body into a U-shape as shown in the illustration.
2. The charcoal tray is set in 3 positions depending on the fuel and application. Set the charcoal tray by inserting the fixing bracket into the insertion hole on the side of the main body.
3. Place the Mezara net in the charcoal tray with the protruding part facing downward.
4. Set the fixing wire of the Gotoku trivet into the slot on the side of the main body.

How To Store

1. Open the main body as shown in the illustration.
2. Put the Mezara net in the charcoal tray, place them on the center of the main body, and fold the left side of the main body to the center.
3. Then fold the right side to the center.
4. Store in the case with the Gotoku trivet.

How To Ignite Fuel

1. Place an appropriate amount of fuel on the Mezara net and ignite it.

(Suggested amount of fuel)

\*Fuel such as charcoal or firewood should be placed in layers and should not excessively touch the sides of the main body.

\*If using a fire lighter, place (spread) it under the fuel to ignite it.

2) Once the fire starts and the heat stabilizes, set the Gotoku trivet according to your application.